
Summer high-speed tyre.
The tyre has protective flanges preventing damage to tyres from curb contact. A thick screening layer and wide breaker enable uniform pressure distribution at the flat spot on wet roads. A stiff metal cord in the breaker and the newest organosilicon filling in the rubber mixture provide low rolling resistance. This enables considerable fuel economy.
